I am astounded at your wisdom!. You must stop the drip, draw a STAT aPTT every two hours until the aPTT is less than 150, then resume the drip at 3 units/kg/hr less and do not rebolus.

I will now reward you with your next clue and another piece of the puzzle.

Script 6